


1)Base Station




Mobile Station




Application server




Allocated the power to the node



Upload file from the mobile station to the base station have ip address as a local host




Data is upload from the base station through nodes



Data is successfully upload



Congestion occur when the node power is low



Data recived at the reciver side.

